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Tyre Changer

Warning
This instruction manual is important for the machine, please read carefully before installation and use; also it is important for safe use and machine maintenance of machine. Please keep this manual properly in order to further maintenance of the machine.
1. Introduction:
Application Range: The semi-automatic tyre changer is especially designed for demounting / mounting tyres from wheel rims.
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Caution：Please use the machine only for purpose for which it is designed, don't use it for other purposes.
Manufacturer shall not be liable for any damage or injury caused by failure to comply with these regulations. 

Safety regulation: Use of this machine is especially reserved to trained and qualified professional persons, those who already read the introduction manual carefully, or someone have the experience for operating similar machinery. Any changes and beyond the scope of use on this machine without manufacturer’s permission or do not according to the manual, may cause the malfunction and damage to machine, manufacturer can cancel warranty coverage for above. If some parts are damaged due to some reason, please replace them according to the spare parts list. (Attention: warranty is one year after manufactures’ delivery date; warranty excludes the easy-broken parts).

2. Warning label and sticking position:

01 Don’t put hands under the Mounting/demounting head during operation; 
02 Don’t put hands between the jaws during operation;

03 Don’t put hands inside the tyre bead when demounting the tyre;

04 Make sure and to check the system is equipped with a good grounding circuit; 
05 Don’t put feet between the Bead Breaker shovel and the body during operation;

Security warning labels
[image: image8]Caution: 
When the security warning labels are defaced or off, please recovery them in time!
Do not allow to operate when the security warning labels are missed or imperfect.    Do not allow to set any objects to obscure the security warning labels.

Clients can self-set the warning labels (as right picture show) at any necessary positions. 

3. Technical data
	locking rim dimensions  
	6~24＂

	Max. Wheel diameter 
	1040mm(41＂)

	Max. Wheel width
	270mm(10＂)

	Working Pressure
	8-10bar

	Power supply  
	110V (1ph)/ 220V (1ph/3ph)/ 380V (3ph)

	Optional Motor power
	0.75/1.1 kw

	Max. Rotating Torque (Turntable)
	1078 Nm

	Overall Dimension  
	96*76*108cm

	Noise Level
	75 Db


Remark: 

Rim dimensions defined at above table are based on the iron wheel rims. Aluminum rims are thicker than the iron wheel rims, so here above rim dimensions are just for the reference.

4. Transport:
When transporting, the machine should be with original package and placed according to the mark on the package. For the already packaged machine should be handled with a corresponding tonnage forklift for loading and unloading. The location to insert the fork feet shown as Fig 1

5. Unpacking & Inspection:
Pull out the nail which is nailed on the plate with tip jaw; unpack the carton and plastic cover. Check and make sure all parts shown on the spare parts list are included. If any parts are missing or broken, please do not use the machine and contact the manufacturer or dealer ASAP.
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                  Fig 1                        Fig 2                                Fig 3
6. Workplace requirements:

Choose workplace in compliance with safety regulations. Connect power supply and air source according to manual and workplace must have good air condition; in order to make the machine run well, its workplace requires at least clear space from each wall shown as Fig 2. If installing it outdoor, it must be protected by roof against rain and sunshine.  
Warning: the machine with motor must not be operated in explosive atmosphere.
[image: image10]7. Position and installation: 
1. Unscrew the nuts at the bottom, position the machine and calibrate it with the horizontal rule. Mount the machine with all the screws and to ensure the machine is stable. Make sure the system is equipped with a good grounding circuit for prevent electric leakage. And have operation range of ground for skid prevention.

2. Unscrew the nut A on the cabinet body B as shown in Fig 3.Lift the column C; mount it on the machine body B by using the nut A through the bolt located on the machine body B. If the column becomes loose after a period of using, tight them immediately. Otherwise the result of damage to the tyre may happen.                        
8. Electricity and Pneumatic connections:
Caution: Before installation and connection, check to be sure that the electricity power supply corresponds to the machine technical data. All the installation of electric and pneumatic devices must be operated by a professional electrician.
Connect the compressed air connector which is on the machine right side with compressed air system. The electric grid that the machine connects to must have fuses protection device and good outer cover grounding protection. Install the leakage automatic air switch on the maim power supply, leakage current is set at 30mA.
Caution: No power plug for this machine, the user should self-connect one power plug no less than 16A as well as in line with the machine voltage. Or directly connect with the power supply according to the above requirements.      
9. Adjusting operation:
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  Turntable Rotation Pedal (Z)
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  Bead Breaker Pedal  (U)
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  Jaws open and close Pedal (V)


Tread the Turntable Rotation Pedal (Z), Turntable (Y) clockwise rotation; Lift up the Turntable Rotation Pedal (Z), Turntable (Y) counterclockwise rotation.
Tread Bead Breaker Pedal (U), Bead Breaker shovel (F) close toward inside; release Bead Breaker Pedal (U), Bead Breaker shovel (F) return to original position.
Tread Jaws open and close Pedal (V), four jaws (G) on the turntable open; tread again, four jaws (G) close. When the pedal is in the middle position, the four jaws stop moving.
Tyre changer operation is consisted of three parts:

1）Breaking the tyre bead
2）Demounting the tyre

[image: image11]3）Mounting the tyre

Caution: Before any operations, don’t wear loose clothing and wear protective hat, gloves, and skid-proof shoes. Ensure to exhaust the air in the tyre completely, and remove all the wheel weights from the rim.

9.1. Breaking the tyre bead：
Ensure to exhaust the air in the tyre completely, place the tyre against the rubber buffer (S). Bring the paddle against the bead about 10mm from the edge of the rim shown as Fig 5. Tread Bead breaker Pedal (U) to push paddle into tyre. Repeat the                Fig5    
above operations on different positions around the tyre and both sides of tyre until tyre bead is released completely.
9.2. Demounting the tyre :
Ensure to remove all the weights on the wheel rim and to exhaust the air in the tyre completely before this operation. Apply lubricating grease (or similar lubricant) around the tyre bead. Without the lubricant may lead to badly wear and tear on tyre. Clamp the wheel methods shown as below regarded to the ruled dimension:

a- to clamp the wheel from outside:

Tread the Jaws open and close Pedal (V) halfway down to middle, positioning for the four clamps (G) by reference scale on the Turntable (Y); put the tyre on turntable, hold the rim, and tread the Jaws open and close Pedal (V) until the wheel is secured by the jaws. 

b- to clamp the wheel from inside: 

Positioning for the four clamps (G) and let them all closed. Put the tyre on the turntable and tread the Jaws open and close Pedal (V) to open the clamps thereby lock the wheel in place.

Caution: Check to make sure the wheel firmly secured by the four clamps before next step.
[image: image12]Lower the Vertical Arm (M) until the Mounting/demounting head (I) rests next to the edge of the rim, flip the Locking Handle to lock the Vertical Arm and Swing Arm in position, and also adjust the Rocker Arm make Mounting/demounting head can raise 2mm-3mm automatically from the edge of the wheel rim. Insert the Lifting Lever (T) between the tyre bead and the front section of the mounting/demounting head (I), and move the tyre above the mounting/demounting head as shown as Fig 6.

                                                                           Fig 6
Caution: Chains, bracelets, loose clothes and anything else close to the rotating parts will bring danger to the operator.
With the Lifting Lever held in position, tread the Turntable Rotation Pedal (Z), rotate the Turntable (Y) in a clockwise direction until the tyre is completely separated from the wheel rim.For the other side tyre demounting, keep using the lifting lever to lift the tyre, make the other side tyre separated from the wheel rim.

9.3. Mounting the tyre :
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Caution: Check to make sure that the tyre and the wheel rim are of same size before mounting the tyre.To avoid any damage on type, lubricate the tyre bead and the wheel rim with the lubrication recommended by manufacturer. Put on the tyre and check the situation.
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Caution: When clamp the wheel rim, don't put your hands on the wheel rim to avoid injury during this operation.

Lock the Hexagonal Vertical Mounting Arm, put the tyre on the rim, let the Rocker Arm back to place as demounting the tyre. And let one side of tyre down bead above the rear section of the Mounting/demounting head, the other side under the front section of the Mounting/demounting head. Suppress the trye with hands or help arm, and then spin the turntable for mounting the tyre down bead.

Repeat the above operation for mounting the tyre up bead. (Fig 7)                    
10. Inflating the tire:
Importance: It is very dangerous during inflating operation, take carefully and comply with instruction. When inflating, it will turn to be extremely dangerous if problems happen to tyre or rim. The possible burst force tire goes upward and outward, the big power may cause injury or death of the operator or the people around.
Tyre may burst caused by following:
1) The wheel rim and the tyre are not of the same size;
2) The tyre or the wheel rim is damaged;
3) The pressure of tyre inflation is over the max. pressure recommended by manufacturer;
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4) The operator fail to comply with the safety regulation;
Please operate as follows:
1) Remove the valve cap from the valve stem;

2) Check to make sure the air nozzle is pressed down completely over the threads of    the valve stem. 

3) Check to make sure that the tyre and the wheel rim are of the same size;

4) Lubricate both the tyre bead and the wheel rim, additional lubrication is required if needed;                                                                        Fig 8

5) Inflate the tyre with break, while inflating, check the pressure listed on the pressure gauge, also check whether the bead is fixed or not. Repeat operation above until the bead is secured; you need take special steps when inflating convex rim or double convex rim;

6) Continue inflating and check the air pressure frequently until to reach the required pressure. 
Notice:

Never exceed the max. inflation pressure given by the tyre manufacturer.
Keep hands and your body away from inflating tyres.
Only specially trained persons are allowed to perform the operations, do not allow other to operate or be near the tyre changer. 
11. Moving machine:

Please use forklift to move the machine. Disconnect the tyre changer from the electricity power supply and pneumatic power supply, lift the base board and insert the feet of forklift. Then mount the tyre changer machine to a new position and fix it tightly.

Notice: the place chosen for fixing the tyre changer must meet the safety regulation.
12. Maintenance:
Caution: disconnect power and air supply before operation

Caution: only the professional persons can do the maintenance. To prolong the machine's life, maintain the machine timely according to the manual. Otherwise, it will impact the reliability of the machine or even cause injury to operator and others nearby.
Caution: before performing any maintenance, disconnect the tyre changer from the electric power supply and pneumatic power supply, and tread the Jaws open and close Pedal or Turntable Rotation Pedal for 3~4 times to evacuate all compressed air from the machine. Damaged parts must be replaced by professional persons with the spare parts provided by manufacturer.                                                               
[image: image16.jpg]


Clean the machine once every day after work. Clean the dirt on the turntable with diesel oil once per week and lubricate the slides and clamps.                           
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Following maintenance must be done at least once per month: Check oil level in Oil Fog Maker, please be filled with SAE30# oil if need. Unscrew with hex wrench (E). Based on connection of compressed air, first to tread Jaws open and close Pedal or Turntable Rotation Pedal 5-6 times, and then check whether oil in Oil Fog Maker drops down a drip of oil. For continuous operation, tread twice every time, drop down a drip of oil, otherwise adjust the screw (D) that controlled oil enter with minus screwdriver. (Fig 9)

As shown in Figure 9-1, when you found there are some water in the cup, push up the drain valve to drain away water with your fingers; loosen your fingers after drained water, drain valve can be automatic closed under the action of the spring.                       
Notice: After the first 20 days of use, retighten the jaws with tightening screws (B) on the Turntable (Fig 10)                                                               
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Notice: in the event of turntable lose power, check to see if the belt is tight as follow steps: Remove the left side cover by unscrewing the screws; adjust two screws located on the motor support, keep a suitable distance between motor support and motor base; tight the screws for the belt tension.(Fig 11)                                       
Caution: please disconnect the machine from electric power supply and pneumatic power supply. 
Notice: If Hexagonal Vertical Arm not be locked or not meet the requirement that 2-3mm from the bottom of Mounting/demounting head to rim, please adjust Hexagonal Locking Plate, refer to Fig 12 and adjust the (X).                             Fig 10
Notice: In order to achieve the reliability of jaws and Bead Breaker shovel, operate as follows to keep their valves clean: 
1. Remove the left side cover of the machine body by unscrewing the two screws; 
2. Loosen the valve Muffler (A) which belong to Jaws open and close Pedal and Bead Breaker Pedal; (A)
3. Clean the silencers with compressed air, please replace it referring to the spare parts list if it is damaged. (Fig 13)
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              Fig 11                        Fig 12
13. Trouble shooting table:
	Problem
	Reason
	Solution

	The turntable rotate just in 

one direction or can’t rotate.
	Reverse Switch broken
	Replace the Reverse Switch

	
	Belt broken 
	Replace the belt 

	
	The Motor’s malfunction
	Check the motor cable or terminal block wire;

Replace the motor if it was broken.

	Demount or fix the wheel, the

turntable can’t lock (spin with

wheel);
The jaws delay to open/close; 
The turntable locks the rim 

incorrectly.
	Leakage of Air network
	Check all the parts on the air network.

	
	The clamping cylinder can’t work.
	Replace the cylinder piston.

	
	Worn jaws
	Replace the jaws.

	
	Broken washers of the chuck cylinder
	Replace it.

	The mounting/demounting head always touch the rim during operation.
	The locking plate incorrectly adjust or unqualified.
	Replace or adjust it.

	
	Screws on the chuck loose; the Hexagonal Vertical Arm can’t be locked by Locking Plate
	Tighten the screws; replace the Locking Plate.

	The Bead Breaker Pedal and Jaw open and close Pedal can’t turn back to the original position.
	 pedal spring broken
	Replace it.

	The Bead Breaker shovel operates difficultly.
	Jammed silencer
	Clean it or replace it.

	
	The washer on the Bead Breaker cylinder is broken.
	Replace it.


14. Guide for ordering spare parts

14.1. Firstly, the damaged or ordered sample should be gained and confirmed the quantity of spare parts

14.2. Confirm the replaced parts specification, avoid wrong order.

The confirmed method showed as following:

According to the use range and place position of parts, find out the codes of parts in the exploded drawing (section 16) from the manual.

For example, if lifting level is needed to be ordered, resulting from the fact that lifting level always placed in the sleeve, and its exploded drawing position is showed as below:
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We can see the code “12” from the picture, then find out all the information of code “12” and record them.

	11
	B-027-060401-0
	Grounding screw M6x40

	12
	C-200-580000-0
	Lifting level

	200-10
	C-200-500000-0
	Bead breaker buffer with pot point


The recorded information:

	12
	C-200-580000-0
	Lifting level


14.3. Gather the detailed information of parts

	Code . 
	Order code 
	Name 
	Qty
	Purchase time of machine

	12
	C-200-580000-0
	Lifting level
	2
	2009.6.25


14.4. Please contact the spare parts department and confirm the order.

14.5. After confirming the order with any problem, the spare parts department will deliver the goods for you according to the order.
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15. Wearing spare parts list

	Code 
	Order code
	Name 
	Code 
	Order code
	Name 

	200-10
	JZ09001023178
	Bead breaker buffer
	331
	FJ08001005151
	O- seal Ø19.6X2.62

	226
	FJ08003005391
	V seal Ø20*28*7.5
	200-426
	DD03009001577
	Reverse switch

	227
	FJ08001005312
	O- seal 63*2.65
	521
	FJ08001005221
	O-seal 30X3.55

	200-228
	JZ09001022841
	Clamping cylinder piston Ø70
	200-522
	JZ09001022990
	Oil resistant seal 

	232
	FJ08001005151
	O- seal Ø19.6X2.62
	200-532
	FJ08001005300
	O-seal 59.9X2.62

	306
	FJ08001005120
	O-seal Ø 16*2.65
	604
	FJ02003003545
	Tyre changer belt A-28

	307
	FJ08001005160
	O-seal Ø 20*2.65
	701
	EQ05001002961
	Inflating gun indicator

	200-308
	FJ08001005146
	O-seal 180x4
	702
	JZ09001022984
	Rubber connection hose

	311
	FJ08003005386
	V-seal 185X168X11.5
	801
	EQ03005002920
	Relief pressure filter 

	200-370
	JZ07001020829
	Bead breaker shovel protection cover(optional)
	804
	EQ03011002941
	Oil fog maker 


16. Exploded drawing:
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	Code 
	Order code
	Name 
	Code 
	Order code
	Name 

	200-1
	JZ08001021107
	machine body 200
	200-10
	JZ09001023178
	Bead breaker buffer with pot point U200

	200-2
	JZ08001021045
	Pedal front cover 200
	11
	FJ04006004049
	screw ST6.3*38

	200-3
	JZ08001021145
	Left cover 200
	12
	JZ09001023041
	Lifting lever 

	4
	FJ04009004668
	hex socket head cap screw M6*10
	200-13
	JZ09001022722
	Bead breaker arm spring U200

	5
	FJ04002003892
	Flat washer 6*14*1.2
	200-14
	JZ09001022719
	Bead breaker arm rubber U200

	6
	FJ04009004879
	Outer hex bolt M8*25
	16
	FJ04009004706
	hex socket head cap screw M8*20

	7
	FJ04009004706
	hex socket head cap screw M8*20
	17
	FJ04002003904
	Flat washer 8*17*1.5

	200-9
	JZ09001023159
	Rubber foot buffer
	239-22
	JZ03001015827
	Oil-water box support U200
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	Code 
	Order code
	Name 

	600-101
	JZ08001021062
	Column U600

	200-102
	JZ09001023188
	Swing arm pin U200

	103
	FJ04009004813
	Outer hex bolt M14*30

	104
	FJ04002003777
	Flat washer 14

	105
	JZ03001015476
	Big washer U200

	200-106
	JZ07001020882
	Column adjust handle U200

	119
	FJ04009004588
	hex socket head cap screw M10*50

	200-120
	JZ07001020885
	Vertical arm cap 200

	200-121
	JZ09001022973
	Vertical arm spring U200 Φ2.8*545

	128
	FJ04002003800
	Flat washer 10*20*2

	130
	FJ04008004444
	Nut M10

	200-133
	JZ03001015654
	Vertical arm 200

	200-134
	JZ09001022967
	Vertical arm washer S36

	136
	JZ03001015342
	Mount/demount head flat washer U200

	137
	FJ04009004770
	Outer hex bolt M10*25

	206-135
	JZ06001020306
	Complete mount/demount head (motorcycle)

	206-139
	JZ09001022698
	mount/demount head 204 

	206-138
	JZ09001015338
	Mount/demount head pulley motorcycle Φ13*13

	200-140
	JZ09001022993
	Hex round pin U200

	141
	FJ04006004059
	screw M12*16

	200-158
	JZ07001020907
	Locking handle cover U200

	200-160
	JZ03001015733
	Locking Handle U200

	200-161
	JZ03001015740
	Locking plate U200

	200-162
	JZ09001023096
	Locking block cover U200

	163
	FJ04002003792
	Flat washer 8

	200-164
	JZ09001023004
	Eccentric shaft nut U200

	165
	FJ04009004879
	Outer hex bolt M8*25

	166
	FJ04008004495
	Nut M12*1.75*T6

	167
	FJ04006004176
	screw M12*30

	200-168
	JZ07001020909
	Locking plate cap

	200-169
	JZ03001015645
	Hex locking board 200

	200-170
	JZ08001021123
	Swing arm U200
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	Code 
	Order code
	Name 

	221-201
	JZ03001015479
	Turntable 630

	200-204
	JZ09001022893
	Jaw 200 

	205
	JZ03001015476
	Big washer U200

	206
	FJ04002003779
	Flat washer 16

	207
	FJ04009004828
	Outer hex bolt M16*40

	208
	JZ07001020860
	Turntable cap U200

	200-209
	JZ03001015610
	Connection rod assembly 540 

	200-210
	JZ03001015453
	Square turntable 540

	211
	JZ03001015457
	Square Turntable Washer 

	212
	FJ04001003757
	Snap Ring 65

	206-214
	JZ03001015836
	Jaw slide guide with pin U206

	215
	FJ04002003813
	Flat washer 12*24*2

	216
	FJ04001003737
	Snap Ring 12

	200-220
	JZ09001015609
	Connection rod nut U200

	206-221
	JZ03001015768
	Jaw slide guide without pin 

	200-222
	JZ09001022929
	Threaded connection rod M8*310

	200-223
	JZ09001022842
	Clamping cylinder piston rod Φ20*320

	224
	JZ09001022837
	Clamping cylinder cover without handle Φ70

	225
	EQ11006003389
	Quick coupler G1/8-Φ8

	226
	FJ08003005391
	V-seal ring Φ20*Φ28*7.5

	227
	FJ08001005312
	O-seal ring Φ63*2.65

	228
	JZ09001022841
	Complete clamping cylinder piston Φ70

	229
	FJ04002003813
	Flat washer 12*24*2

	230
	FJ04008004495
	Nut M12*1.75*T6

	200-231
	JZ09001022851
	Clamping cylinder barrel Φ70*279

	232
	FJ08001005151
	O-seal ring Φ19.6*2.62

	233
	JZ09001022839
	Clamping cylinder cover with handle Φ70

	234
	EQ11005003366
	Quick coupler G1/8-Φ8

	235
	FJ04008004459
	Nut M8

	200-236
	JZ06001020234
	Complete clamping cylinder Φ70*279

	206-242
	JZ03001015536
	Sliding track U206

	206-243
	JZ09001022687
	Pin handle M8*SR12.5

	206-244
	JZ09001015539
	Sliding track plate 

	245
	FJ04009004806
	Outer hex bolt M12*65

	206-246
	JZ03001015531
	Sliding track block U-206

	250
	JZ09001022807
	Fixing pin spring Φ2*54
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	Code 
	Order code
	Name 
	Code 
	Order code
	Name 

	200-13
	JZ09001022722
	Bead breaker arm spring U200
	317
	FJ04008004517
	Nut M16*1.5

	200-301
	JZ09001011179
	Hex socket head bolt M14*30
	318
	CF03003001068
	Guide belt 10*2

	302
	FJ04008004458
	Nut M6
	200-370
	JZ07001020831
	Bead breaker shovel protection coverU206 (optional)

	303
	EQ11005003350
	Quick coupler G1/4-Φ8
	319
	FJ04002003777
	Flat washer 14

	304
	FJ04008004517
	Nut M16*1.5
	358
	JZ09001023166
	Spring U2098

	305
	FJ04002003833
	Flat washer 16*28*2
	320
	FJ04001003741
	Snap Ring 16

	306
	FJ08001005120
	O-seal ring Φ16*2.65
	200-321
	FJ08001005146
	O-seal ring Φ180*4

	307
	FJ08001005160
	O-seal ring Φ20*2.65
	200-322
	JZ08001021156
	Bead breaker arm 200

	200-308
	FJ08001005135
	O-seal ring Φ170.8*5.33
	200-323
	JZ03001015349
	Bead breaker arm pin U200

	200-309
	JZ03001015378
	Bead breaker cylinder cover assembly D186
	200-324
	JZ03001015382
	Bead breaker cylinder rotating pin U200

	200-310
	JZ09001022746
	Bead  breaker cylinder piston rod D186
	325
	FJ04002003813
	Flat washer 12*24*2

	311
	FJ08003005386
	V-seal ring Φ185*Φ168* 10.8(+0.1/-0.3)
	326
	FJ04008004445
	Nut M12

	200-312
	JZ09001022744
	Bead breaker cylinder piston Φ185
	327
	FJ04002003915
	Flat washer 8*30*3

	200-313
	JZ09001015384
	Bead breaker cylinder barrel U200
	328
	FJ04002003792
	Flat washer 8

	314
	FJ04009004676
	hex socket head cap screw M6*16
	329
	FJ04009004877
	Outer hex bolt M8*20

	200-315
	JZ03001015790
	Bead breaker shovel assembly T/6
	330
	EQ11006003389
	Quick coupler G1/8-Φ8

	316
	FJ04009004613
	hex socket head cap screw M12*90
	200-334
	JZ06001020265
	Complete bead breaker cylinder U200
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	Code 
	Order code
	Name 
	Code 
	Order code
	Name 

	200-401
	JZ09001022773
	Reverse switch pedal 1#
	428
	FJ04002003890
	Flat washer 6*12*1

	221-402
	JZ09001023136
	5-way valve pedal(right) 3#
	429
	FJ04002003874
	Flat washer 4*8*0.5

	405
	FJ04001003737
	Snap Ring 12
	430
	FJ04006004323
	screw M4*16

	406
	FJ04002003813
	Flat washer 12*24*2
	200-431
	JZ07001020856
	Reverse switch handle 

	407
	FJ04006004200
	screw M4*30
	432
	FJ04008004458
	Nut M6

	408
	FJ04002003874
	Flat washer 4*8*0.5
	433
	FJ04002003859
	Flat washer 3*6*0.5

	409
	FJ04008004455
	Nut M4
	434
	FJ04006004306
	screw M3*16

	410
	FJ04008004459
	Nut M8
	200-435
	JZ03001015560
	Pedal Connection Rod 

	411
	FJ04002003904
	Flat washer 8*17*1.5
	437
	JZ03001015570
	Pedal front shaft 

	200-412
	JZ07001020913
	Cam connection rod 
	438
	FJ04008004515
	Nut M8

	200-413
	JZ09001022882
	Pedal suport board 
	439
	JZ09001022873
	Pedal twist spring 

	200-414
	JZ09001022872
	Pedal Spring U200
	440
	FJ04009004715
	hex socket head cap screw M8*50

	200-415
	JZ07001020914
	Cam U200
	441
	FJ04009004706
	hex socket head cap screw M8*20

	200-416
	JZ09001023109
	Cam washer 0.5
	442
	EQ10004003264
	Quick coupler G1/8-Φ8

	417
	FJ04009004680
	hex socket head cap screw M6*20
	445
	EQ10001003242
	Quick coupler G1/8-2*Φ8

	418
	FJ04002003890
	Flat washer 6*12*1
	200-449
	JZ07001020920
	5-way valve barrel U200

	420
	FJ04006004228
	screw ST2.9*12
	200-451
	JZ07001020918
	5-way valve cover U6603

	200-421
	JZ03001015747
	Cam cover U200
	452
	FJ04006004372
	screw ST2.9*14

	422
	JZ06001020282
	5-way valve (L-union,without rod) 
	453
	EQ04002002955
	Muffler G1/8

	423
	JZ06001020283
	5-way valve (T-union,without rod) 
	200-455
	JZ09001015771
	5-way valve rod 

	200-424
	JZ07001020853
	Reverse Switch Cover 
	200-456
	JZ07001020919
	5-way valve rod spacer 

	425
	FJ04008004511
	Nut M4
	457
	FJ08001005087
	O-seal ring Φ12*20*4

	200-426
	DD03009001577
	Reverse switch LW8-25N2/5.5
	200-480
	JZ06001020268
	Complete 3-pedals assembly 200

	427
	FJ04009004680
	hex socket head cap screw M6*20
	
	
	





	Code 
	Order code
	Name 

	200-501
	JZ09001022681
	Gear box lower cover U300

	502
	FJ02010003613
	Bearing 30204

	503
	FJ08007005413
	Gear Seal Φ20*Φ35*8

	200-504
	JZ09001023119
	Gear Belt pulley U200

	505
	FJ04009004879
	Outer hex bolt M8*25

	506
	FJ06001004964
	Key washer 6*20

	200-507
	JZ09001023118
	Worm rod Φ42*218

	508
	FJ02010003623
	Bearing 6010-2RS

	200-509
	JZ09001023126
	Worm gear shaft Φ50*280

	200-510
	JZ09001023250
	Worm gear U200

	200-511
	JZ02007011727
	spacer U200

	512
	FJ04009004779
	Outer hex bolt M10*55

	513
	FJ04002003773
	Flat washer 10

	200-514
	FJ06002005000
	Pin Φ6*20

	515
	FJ04002003800
	Flat washer 10*20*2

	516
	FJ04009004680
	hex socket head cap screw M6*20

	200-518
	JZ09001022679
	Gear box upper cover U300

	519
	FJ06001004962
	Key washer 10*40

	520
	FJ06001004963
	Key washer 14*40

	521
	FJ08001005221
	O-seal ring Φ30*3.55

	200-522
	JZ09001022990
	oil resistant seal U200

	200-526
	JZ06001020255
	Complete gear box 
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	Code 
	Order code
	Name 

	A04
	EQ11002003333
	T-union 3*Φ8

	A44
	FJ04009004676
	Hex socket head bolt M6*16

	A48
	EQ11002003340
	T-union G1/8-2*8

	200-531
	JZ02007015872
	Rotating valve casing U200

	200-532
	FJ08001005300
	O-seal Φ59.9*2.62

	200-535
	JZ02007015676
	Rotating valve mandrel U200

	537
	CF01002000936
	Hose Φ8*Φ5*10m

	A41
	EQ11006003389
	Straight union 1/8-Ø8

	548
	FJ04006004060
	Hex socket head bolt M4X6

	200-540
	JZ06001020249
	Complete Rotating valve U200
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	Code 
	Order code
	Name 

	200-504
	JZ09001023119
	Gear Belt pulley U200 U200

	601-MC
	Decide order according to customer's requirement：

___V/___HZ/___KW/___PH

For example：220-240V/50HZ/0.75KW/1PH

	601-MY
	

	200-602
	JZ09001015421
	Motor Belt pulley U200

	603
	FJ04006004178
	screw M8*12

	604
	FJ02003003545
	Balancer Belt A-686

	605
	FJ04009004889
	Outer hex bolt M8*65

	606
	FJ04002003915
	Flat washer 8*30*3

	607-80
	DD04009001964
	capacitance 80uF/250V

	607-50
	DD04009001883
	capacitance 50uF/450V

	608
	FJ04002003800
	Flat washer 10*20*2

	609
	FJ04002003773
	Flat washer 10

	610
	FJ04009004770
	Outer hex bolt M10*25

	611
	FJ04009004883
	Outer hex bolt M8*35

	612
	FJ04008004515
	Nut M8

	613
	FJ04002003910
	Flat washer 8*22*2

	614
	JZ09001022782
	Motor Rubber Buffer 10*30*4

	200-615
	JZ03001015423
	Motor support 0.75KW/1.1KW

	616
	JZ12001026447
	Motor Cable 220V RVV5*1.5 0.7m

	617
	FJ04002003792
	Flat washer 8

	200-618
	JZ09001022782
	Motor Rubber Buffer 10*30*4

	200-504
	JZ09001023119
	Gear Belt pulley U200
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	701
	EQ05001002961
	Digital inflating gun 0-10Bar/TG-7

	702
	JZ09001022984
	Helical hose 8*5*2500

	703
	EQ14003003478
	Notch nut G1/4

	704
	EQ07005003072
	Straight union 2*G1/4 external thread 

	705
	FJ04002003822
	Flat washer 13*24*1

	706
	EQ03003002911
	Pressure adjust valve AR2000-G1/4

	707
	EQ10004003257
	Quick coupler G1/4-Φ8

	708
	
	Complete inflating gun,without preasure adjust valve

	708W
	JZ06001020203
	Complete inflating gun,with preasure adjust valve
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	802
	Decide by Type of Quick nozzle
	Quick nozzle

	841
	EQ11005003350
	Quick coupler G1/4-Φ8

	842
	EQ03001002905
	Filter AW+AL2000

	
	CF01002000915
	Air hose Φ8*Φ5

	840
	Decide by Type of Quick nozzle
	Complete oil fog maker 2000
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17. Circuit diagram:
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18. Pneumatic drawing: 
Fig 4 





Fig 7





Fig 9





Fig 9-1
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Fig 13





Special statement


◆Manufacturer reserves the rights to change the parts specification without beforehand notice for the users.


◆Manufacturer do not liable for the modification and improvement of the products which have been sale
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